**CT and MRI scanning of cetaceans for blast injury and Anatomy studies.**

Diagnostic Health Imaging Center

**Diagnostic Health Anchorage**
4100 Lake Otis Parkway, Suite 102
Anchorage, AK 99508
**Phone:** 907-729-5800
**Fax:** 907-729-5889

Dr. Harold Cable

David Joslin facility Manager

Alaska Spine Institute **Imaging Center**

**Dr. Harold Cable and Dr. John McCormick**

**Stan at 907 982-7978**

Phone: 907.677.4700Fax: 907.677.4720
3801 University Lake Drive, Anchorage, AK 99508
appts@alaskaspineinstitute.com

24” bore diameter MRI

**Alaska Innovative Imaging**

|  |
| --- |
| 2110 East Northern Lights BoulevardAnchorage, AK 99508(907) 561-7318Carrie said they have some some studies for them….  |

**CT imaging**

Dorsal fin may present an object to scanning. Fin can be taped down or removed by cutting.

Imaging protocol multi slice scanner:

Best case image capture is 0.5mm slices through entire body (tip to tail). However, if this is not feasible:

0.5mm slice thickness through each individual ear, axial scan mode, bone reconstruction algorithm only

0.5- 3 mm slice thickness through the entire head and 0.5-3mm slices thickness through the thorax and abdomen using soft tissue and bone reconstruction algorithms. Helical scan mode can be used (pitch equivalent to single slice pitch of 1.4-1.7)

Imaging protocol single slice scanner:

1 mm slices through entire body (tip to tail). However, if this is not feasible:

1 mm slice thickness through each individual ear (if possible) or both ears simultaneously, bone reconstruction algorithm only

1-3mm slice thickness through the head and1- 3mm slice thickness through the thorax and abdomen using soft tissue and bone reconstruction algorithms. Helical scan mode can be used with pitch 1.4-1.7

**MR Imaging –GE  3T (?)**

Images acquired in the axial (human coronal) plane. T2 weighted images

Do all three directions in 2D (if  time feasible)

Imaging protocol parameters: slice thickness = 0.7 mm, slice interleave (interval) = 0 mm, Time to repetition (TR) = 3000 ms, Time to echo (TE) = 13 ms, field of view = 150 mm, matrix = 256 × 256 pixels.

Alternative (whole body)3-D FSPGR protocol: TR-8.1; TE 3.2; Bandwidth 31.3; Inversion time 600 1mm slices with 0 space interval; Field of View 28 x 22; Matrix 256 x 256

Judy St. Leger, DVM, DACVP

SeaWorld Parks and Entertainment

500 SeaWorld Dr.

San Diego, CA 92109

Judy.st.leger@seaworld.com

619-225-4259 (W1)

619-563-6708 (W2)

518-993-4983 (W3)